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	JABATAN PENGAIRAN DAN SALIRAN NEGERI SELANGOR

	Sebut Harga untuk kerja JPS Negeri Selangor

	

	Kepada :
	Tawaran Harga  : BPBRB    

	
	No. Sebut Harga: JPS/P/BPBRB/P(33)/29/2026(SH)

	         
	Rujukan Fail : JPS.SEL.015/1/32 Jld.    (       )

	           
	Borang Tawaran dikeluarkan oleh :

	
	Ketua Bahagian

	
	Bahagian Pengurusan Banjir dan Reka Bentuk (BPBRB) JPS Negeri Selangor

	
	

	
	Tarikh : 18 September 2026

	
	

	Sila sebutkan tawaran harga bagi mengadakan segala bahan-bahan, peralatan, jentera dan tenaga buruh serta mengikut syarat-syarat yang ditentukan bagi: 

	

	KERJA-KERJA PENYIASATAN TANAH BAGI REKABENTUK TERPERINCI RANCANGAN TEBATAN BANJIR SUNGAI LANGAT FASA 2, SELANGOR - PAKEJ 1: DAERAH HULU LANGAT

	

	Tawaran akan ditutup pada 12.00 tengahari  5hb Oktober 2026 di Pejabat Pengarah Pengairan dan Saliran Negeri Selangor, Tingkat 5, Blok Podium Selatan, Bangunan Sultan Salahuddin Abdul Aziz Shah, 40626 Shah Alam, Selangor Darul Ehsan. Tawaran hendaklah di masukkan kedalam sampul surat bermeteri yang di tandakan di sudut kanan Rujukan Sebutharga.

	Bil
	Perkara
	Unit
	Kuantiti
	Kadar                  (RM)
	Harga                  (RM)

	1.0
	GENERAL CONDITIONS AND PRELIMINARIES
	
	
	
	

	
	
	
	
	
	

	1.1
	Allow for compliance with the terms of each of the Conditions of Contract.
	Lump Sum
	
	
	

	
	
	
	
	
	

	1.2
	Allow for compliance with the terms of the 
Specification.
	Lump Sum
	
	
	

	
	
	
	
	
	

	1.3
	Allow for compliance with the terms of the Preambles of the Bill of Quantities.
	Lump Sum
	
	
	

	
	
	
	
	
	

	1.4
	Allow for compliance with the terms of additional conditions as given applicable to this particular project.
	Lump Sum
	
	
	

	
	
	
	
	
	

	1.5
	Allow for provision of full time professional attendence on site for the duration of the contract.
	Lump Sum
	
	
	

	
	
	
	
	
	

	1.6
	Provide two (2) number copies of Interim Factual Report.
	Lump Sum
	
	
	

	
	
	
	
	
	

	1.7
	Provide six (6) number copies of complete Final Factual Report, one compiled and bound set of all raw field and Laboratory sheets and one copy of Factual Report in electronics format.
	Lump Sum
	
	
	

	
	
	
	
	
	

	1.8
	Allow for Licensed Surveyor for setting up of all test locations and take levels.
	Lump Sum
	
	
	

	
	
	
	
	
	

	1.9
	Allow for provision of photographs in electronic.
	Lump Sum
	
	
	

	
	
	
	
	
	

	1.10
	Provide additional copies of final factual report.
	No.
	Rate Only
	
	

	
	
	
	
	
	

	TOTAL OF BILL NO.1 CARRIED TO SUMMARY
	


	Bil
	Perkara
	Unit
	Kuantiti
	Kadar                  (RM)
	Harga                  (RM)

	
	
	
	
	
	

	2.0
	SUNGAI LANGAT
	
	
	
	

	
	
	
	
	
	

	2.1
	BORING PLANT - MOBILIZATION
	
	
	 
	 

	
	
	
	
	
	

	2.1.1
	Bring the boring plant to the site and remove the same from site after completion of boring , shall include erecting the boring plant including materials, installation, dismantling and removal from site after completion.
	Lump Sum
	
	
	

	
	
	
	
	
	

	2.1.2
	Move the boring plant from one borehole position to the next, including dismantling it at the old position.
	Movement
	67
	
	

	
	
	
	
	
	

	
	BORING IN SOIL
	
	
	
	

	
	
	
	
	
	

	2.2
	Rotary Wash Boring
	
	
	
	

	
	Carry out rotary wash boring whether cased or uncased, using water as flushing medium or as otherwise specified by Employer.
	
	
	
	

	
	
	
	
	
	

	2.2.1
	Depth from existing ground level not exceeding (n.e) 10m.
	Metre
	680
	
	

	
	
	
	
	
	

	2.2.2
	- Ditto - exceeding 10m but n.e 20m
	Metre
	680
	
	

	
	
	
	
	
	

	2.2.3
	- Ditto - exceeding 20m but n.e 30m
	Metre
	680
	
	

	
	
	
	
	
	

	2.2.4
	- Ditto - exceeding 30m but n.e 40m
	Metre
	260
	
	

	
	
	
	
	
	

	2.3
	Rotary Core Drilling
	
	
	
	

	
	Carry out diamond rotary rock core drilling.
	
	
	
	

	
	
	
	
	
	

	2.3.1
	Depth from existing ground level not exceeding (n.e) 10m.
	Metre
	120
	
	

	
	
	
	
	
	

	2.3.2
	- Ditto - exceeding 10m but n.e 20m
	Metre
	120
	
	

	
	
	
	
	
	

	2.3.3
	- Ditto - exceeding 20m but n.e 30m
	Metre
	168
	
	

	
	
	
	
	
	

	2.3.4
	- Ditto - exceeding 30m but n.e 40m
	Metre
	156
	
	

	
	
	
	
	
	

	2.4
	Standard Penetration Test (SPT)
	
	
	
	

	
	
	
	
	
	

	2.4.1
	River (32 Boreholes)
	
	
	
	

	
	Carry out standard penetration test
	
	
	
	

	
	
	
	
	
	

	2.4.1.1
	Depth from existing ground level not exceeding (n.e) 10m.
	No.
	192
	
	

	
	
	
	
	
	

	2.4.1.2
	- Ditto - exceeding 10m but n.e 20m
	No.
	224
	
	

	
	
	
	
	
	

	2.4.1.3
	- Ditto - exceeding 20m but n.e 30m
	No.
	224
	
	

	
	
	
	
	
	

	2.4.2
	Bridge (21 Boreholes)
	
	
	
	

	
	Carry out standard penetration test
	
	
	
	

	
	
	
	
	
	


	Bil
	Perkara
	Unit
	Kuantiti
	Kadar                  (RM)
	Harga                  (RM)

	
	
	
	
	
	

	2.4.2.1
	Depth from existing ground level not exceeding (n.e) 10m.
	No.
	126
	
	

	
	
	
	
	
	

	2.4.2.2
	- Ditto - exceeding 10m but n.e 20m
	No.
	147
	
	

	
	
	
	
	
	

	2.4.2.3
	- Ditto - exceeding 20m but n.e 30m
	No.
	147
	
	

	
	
	
	
	
	

	2.4.2.4
	- Ditto - exceeding 30m but n.e 40m
	No.
	147
	
	

	
	
	
	
	
	

	2.4.3
	Pond (10 Boreholes)
	
	
	
	

	
	Carry out standard penetration test.
	
	
	
	

	
	
	
	
	
	

	2.4.3.1
	Depth from existing ground level not exceeding (n.e) 10m.
	No.
	60
	
	

	
	
	
	
	
	

	2.4.3.2
	- Ditto - exceeding 10m but n.e 20m
	No.
	70
	
	

	
	
	
	
	
	

	2.4.3.3
	- Ditto - exceeding 20m but n.e 30m
	No.
	70
	
	

	
	
	
	
	
	

	2.4.4
	Control Gate Structure (5 Boreholes)
	
	
	
	

	
	Carry out standard penetration test
	
	
	
	

	
	
	
	
	
	

	2.4.4.1
	Depth from existing ground level not exceeding (n.e) 10m.
	No.
	30
	
	

	
	
	
	
	
	

	2.4.4.2
	- Ditto - exceeding 10m but n.e 20m
	No.
	35
	
	

	
	
	
	
	
	

	2.4.4.3
	- Ditto - exceeding 20m but n.e 30m
	No.
	35
	
	

	
	
	
	
	
	

	2.4.4.4
	- Ditto - exceeding 30m but n.e 40m
	No.
	35
	
	

	
	
	
	
	
	

	
	SAMPLING
	
	
	
	

	
	
	
	
	
	

	2.5
	Disturbed Samples
	
	
	
	

	
	Obtain disturbed samples from split-barrel tube or as otherwise specified by Employer.
	
	
	
	

	
	
	
	
	
	

	2.5.1
	Depth from existing ground level not exceeding (n.e) 10m.
	No.
	408
	
	

	
	
	
	
	
	

	2.5.2
	- Ditto - exceeding 10m but n.e 20m
	No.
	476
	
	

	
	
	
	
	
	

	2.5.3
	- Ditto - exceeding 20m but n.e 30m
	No.
	476
	
	

	
	
	
	
	
	

	2.5.4
	- Ditto - exceeding 30m but n.e 40m
	No.
	182
	
	

	
	
	
	
	
	

	2.6
	Undisturbed Samples Thin-walled
	
	
	
	

	
	Obtain thin-walled undisturbed samples in soft to from firm soil with minimum 75mm outside diameter and nominal length of 1000mm.
	
	
	
	

	
	
	
	
	
	

	2.6.1
	Depth from existing ground level not exceeding (n.e) 10m.
	No.
	136
	
	

	
	
	
	
	
	

	2.6.2
	- Ditto - exceeding 10m but n.e 20m
	No.
	68
	
	

	
	
	
	
	
	

	2.6.3
	- Ditto - exceeding 20m but n.e 30m
	No.
	Rate Only
	
	

	
	
	
	
	
	


	Bil
	Perkara
	Unit
	Kuantiti
	Kadar                  (RM)
	Harga                  (RM)

	2.7
	Cone Penetration Test - Mechanical
	
	
	
	

	
	Carry out cone penetration test or "Dutch Cone" in accordance with ASTM 3441.
	
	
	
	

	
	
	
	
	
	

	2.7.1
	Mobilisation of all plants and equipments to the site including transfer between different locations within the site, handling, assembling and demobilisation upon completion.
	Lump Sum
	
	
	

	
	
	
	
	
	

	2.7.2
	Shifting of plant and equipment from one borehole position to the next borehole position, rate to include dismantling from one position and erecting at another position where the borehole is to be carried out on.
	No.
	29
	
	

	
	
	
	
	
	

	2.7.3
	Depth from existing ground level not exceeding (n.e) 10m.
	Metre
	300
	
	

	
	
	
	
	
	

	2.7.4
	- Ditto - exceeding 10m but n.e 20m
	Metre
	300
	
	

	
	
	
	
	
	

	2.7.5
	- Ditto - exceeding 20m but n.e 30m
	Metre
	300
	
	

	
	
	
	
	
	

	2.8
	Classification Test
	
	
	
	

	
	Carry out classification tests in accordance with BS 1377:Part 2:1990 or as otherwise specified by Employer.
	
	
	
	

	
	
	
	
	
	

	2.8.1
	Moisture Content (Method 3)
	No.
	771
	
	

	
	
	
	
	
	

	2.8.2
	Liquid Limit            }
	No.
	771
	
	

	
	
	
	
	
	

	2.8.3
	Plastic Limit           }    (Method 4 & 5)
	No.
	771
	
	

	
	
	
	
	
	

	2.8.4
	Plasticity Index      }
	No.
	771
	
	

	
	
	
	
	
	

	2.8.5
	Specific Gravity (Method 8)
	No.
	771
	
	

	
	
	
	
	
	

	2.8.6
	Linear Shrinkage (Method 6)
	No.
	771
	
	

	
	
	
	
	
	

	2.8.7
	Particle size distribution for coarse-grained soil wet sieving (Method 9.2)
	No.
	771
	
	

	
	
	
	
	
	

	2.8.8
	Particle size distribution for fine-grained soil - hydrometer (Method 9.5)
	No.
	771
	
	

	
	
	
	
	
	

	2.9
	Compressibility Test
	
	
	
	

	
	Carry out compressibility tests in accordance with BS 1377: Part 5: 1990
	
	
	
	

	
	
	
	
	
	

	2.9.1
	Determine one-dimensional consolidation characteristics using oedometer (Method 3)
	No.
	50
	
	

	
	
	
	
	
	

	2.10
	Strength Test on Soil
	
	
	
	

	
	
	
	
	
	

	2.10.1
	Unconsolidated Undrained Triaxial Test on a 38mm dia specimen (3 speciment)
	Nos.
	100
	
	

	
	
	
	
	
	

	2.10.2
	Consolidated Undrained Triaxial Test (CIU) with pore pressure and volume change measurement on a set of 3 specimen of 38mm diameter samples
	Nos.
	50
	
	

	
	
	
	
	
	


	Bil
	Perkara
	Unit
	Kuantiti
	Kadar                  (RM)
	Harga                  (RM)

	2.11
	Rock Compression Test
	
	
	
	

	
	
	
	
	
	

	2.11.1
	Carry out unconfined rock compression test on the core sample.
	Nos.
	70
	
	

	
	
	
	
	
	

	TOTAL OF BILL NO.2 CARRIED TO SUMMARY
	


	Bil
	Perkara
	Unit
	Kuantiti
	Kadar                  (RM)
	Harga                  (RM)

	3.0
	SUNGAI LUI
	
	
	
	

	
	
	
	
	
	

	3.1
	BORING PLANT - MOBILIZATION
	
	
	
	

	
	
	
	
	
	

	3.1.1
	Bring the boring plant to the site and remove the same from site after completion of boring , shall include erecting the boring plant including materials, installation, dismantling and removal from site after completion.
	Lump Sum
	
	
	

	
	
	
	
	
	

	3.1.2
	Move the boring plant from one borehole position to the next, including dismantling it at the old position.
	Movement
	5
	
	

	
	
	
	
	
	

	3.2
	Rotary Wash Boring
	
	
	
	

	
	Carry out rotary wash boring whether cased or uncased, using water as flushing medium or as otherwise specified by Employer.
	
	
	
	

	
	
	
	
	
	

	3.2.1
	Depth from existing ground level not exceeding (n.e) 10m.
	Metre
	60
	
	

	
	
	
	
	
	

	3.2.2
	- Ditto - exceeding 10m but n.e 20m
	Metre
	60
	
	

	
	
	
	
	
	

	3.2.3
	- Ditto - exceeding 20m but n.e 30m
	Metre
	60
	
	

	
	
	
	
	
	

	3.2.4
	- Ditto - exceeding 30m but n.e 40m
	Metre
	10
	
	

	
	
	
	
	
	

	3.3
	Rotary Core Drilling
	
	
	
	

	
	Carry out diamond rotary rock core drilling.
	
	
	
	

	
	
	
	
	
	

	3.3.1
	Depth from existing ground level not exceeding (n.e) 10m.
	Metre
	42
	
	

	
	
	
	
	
	

	3.3.2
	- Ditto - exceeding 10m but n.e 20m
	Metre
	42
	
	

	
	
	
	
	
	

	3.3.3
	- Ditto - exceeding 20m but n.e 30m
	Metre
	42
	
	

	
	
	
	
	
	

	3.3.4
	- Ditto - exceeding 30m but n.e 40m
	Metre
	6
	
	

	
	
	
	
	
	

	3.4
	Standard Penetration Test (SPT)
	
	
	
	

	
	
	
	
	
	

	3.4.1
	River (5 Boreholes)
	
	
	
	

	
	Carry out standard penetration test
	
	
	
	

	
	
	
	
	
	

	3.4.1.1
	Depth from existing ground level not exceeding (n.e) 10m.
	No.
	30
	
	

	
	
	
	
	
	

	3.4.1.2
	- Ditto - exceeding 10m but n.e 20m
	No.
	35
	
	

	
	
	
	
	
	

	3.4.1.3
	- Ditto - exceeding 20m but n.e 30m
	No.
	35
	
	

	
	
	
	
	
	

	3.4.2
	Bridge (1 Boreholes)
	 
	
	
	

	
	Carry out standard penetration test 
	 
	
	
	

	
	 
	 
	
	
	

	3.4.2.1
	Depth from existing ground level not exceeding (n.e) 10m.
	No.
	6
	
	

	
	
	
	
	
	

	3.4.2.2
	 - Ditto - exceeding 10m but n.e 20m
	No.
	7
	
	

	
	 
	 
	
	
	


	Bil
	Perkara
	Unit
	Kuantiti
	Kadar                  (RM)
	Harga                  (RM)

	3.4.2.3
	 - Ditto - exceeding 20m but n.e 30m
	No.
	7
	
	

	
	
	
	
	
	

	3.4.2.4
	- Ditto - exceeding 20m but n.e 30m
	No.
	7
	
	

	
	
	
	
	
	

	
	SAMPLING
	
	
	
	

	
	
	
	
	
	

	3.5
	Disturbed Samples
	
	
	
	

	
	Obtain disturbed samples from split-barrel tube or as otherwise specified by Employer.
	
	
	
	

	
	
	
	
	
	

	3.5.1
	Depth from existing ground level not exceeding (n.e) 10m.
	No.
	36
	
	

	
	
	
	
	
	

	3.5.2
	- Ditto - exceeding 10m but n.e 20m
	No.
	42
	
	

	
	
	
	
	
	

	3.5.3
	- Ditto - exceeding 20m but n.e 30m
	No.
	42
	
	

	
	
	
	
	
	

	3.5.4
	- Ditto - exceeding 30m but n.e 40m
	No.
	7
	
	

	
	
	
	
	
	

	3.6
	Undisturbed Samples Thin-walled
	
	
	
	

	
	Obtain thin-walled undisturbed samples in soft to from firm soil with minimum 75mm outside diameter and nominal length of 1000mm.
	
	
	
	

	
	
	
	
	
	

	3.6.1
	Depth from existing ground level not exceeding (n.e) 10m.
	No.
	12
	
	

	
	
	
	
	
	

	3.6.2
	- Ditto - exceeding 10m but n.e 20m
	No.
	6
	
	

	
	
	
	
	
	

	3.6.3
	- Ditto - exceeding 20m but n.e 30m
	No.
	Rate Only
	
	

	
	
	
	
	
	

	3.7
	Cone Penetration Test - Mechanical
	
	
	
	

	
	Carry out cone penetration test or "Dutch Cone" in accordance with ASTM 3441.
	
	
	
	

	
	
	
	
	
	

	3.7.1
	Mobilisation of all plants and equipments to the site including transfer between different locations within the site, handling, assembling and demobilisation upon completion.
	Lump Sum
	
	
	

	
	
	
	
	
	

	3.7.2
	Shifting of plant and equipment from one borehole position to the next borehole position, rate to include dismantling from one position and erecting at another position where the borehole is to be carried out on.
	No.
	8
	
	

	
	
	
	
	
	

	3.7.3
	Depth from existing ground level not exceeding (n.e) 10m.
	Metre
	90
	
	

	
	
	
	
	
	

	3.7.4
	- Ditto - exceeding 10m but n.e 20m
	Metre
	90
	
	

	
	
	
	
	
	

	3.7.5
	- Ditto - exceeding 20m but n.e 30m
	Metre
	90
	
	

	
	
	
	
	
	

	3.8
	Classification Test
	
	
	
	

	
	Carry out classification tests in accordance with BS 1377:Part 2:1990 or as otherwise specified by Employer.
	
	
	
	

	
	
	
	
	
	

	3.8.1
	Moisture Content (Method 3)
	No.
	64
	
	

	
	
	
	
	
	


	Bil
	Perkara
	Unit
	Kuantiti
	Kadar                  (RM)
	Harga                  (RM)

	
	
	
	
	
	

	3.8.2
	Liquid Limit            }
	No.
	64
	
	

	
	
	
	
	
	

	3.8.3
	Plastic Limit           }    (Method 4 & 5)
	No.
	64
	
	

	
	
	
	
	
	

	3.8.4
	Plasticity Index      }
	No.
	64
	
	

	
	
	
	
	
	

	3.8.5
	Specific Gravity (Method 8)
	No.
	64
	
	

	
	
	
	
	
	

	3.8.6
	Linear Shrinkage (Method 6)
	No.
	64
	
	

	
	
	
	
	
	

	3.8.7
	Particle size distribution for coarse-grained soil wet sieving (Method 9.2)
	No.
	64
	
	

	
	
	
	
	
	

	3.8.8
	Particle size distribution for fine-grained soil - hydrometer (Method 9.5)
	No.
	64
	
	

	
	
	
	
	
	

	3.9
	Compressibility Test
	
	
	
	

	
	Carry out compressibility tests in accordance with BS 1377: Part 5: 1990
	
	
	
	

	
	
	
	
	
	

	3.9.1
	Determine one-dimensional consolidation characteristics using oedometer (Method 3)
	No.
	12
	
	

	
	
	
	
	
	

	3.10
	Strength Test on Soil
	
	
	
	

	
	
	
	
	
	

	3.10.1
	Unconsolidated Undrained Triaxial Test on a 38mm dia specimen (3 speciment)
	Nos.
	12
	
	

	
	
	
	
	
	

	3.10.2
	Consolidated Undrained Triaxial Test (CIU) with pore pressure and volume change measurement on a set of 3 specimen of 38mm diameter samples
	Nos.
	6
	
	

	
	
	
	
	
	

	3.11
	Rock Compression Test
	
	
	
	

	
	
	
	
	
	

	3.11.1
	Carry out unconfined rock compression test on the core sample.
	Nos.
	6
	
	

	
	
	
	
	
	

	TOTAL OF BILL NO.3 CARRIED TO SUMMARY
	

	GRAND TOTAL OF BILL (NO.1 + NO.2 + NO.3)
	


Lampiran A
SYARAT-SYARAT

1.
Kontraktor dianggap telah melawat dan mengetahui akan tempat kerja yang dijalankan dan berpuashati dengan syarat-syarat yang dikenakan dan mengkaji dengan terperinci masalah yang akan timbul bersabit dengan kerja ini supaya tidak menjejaskan kerja. Segala tuntutan yang bersabit dengan kerja ini tidak boleh dibuat dan tidak akan dilayan.
2.
Kontraktor yang berjaya hendaklah memulakan kerja dalam tempoh 7 hari dari tarikh surat tawaran dan hendaklah mengikut arahan dan kelulusan Pegawai Penguasa JPS Negeri Selangor atau wakilnya.

a) Jika Kontraktor gagal memulakan kerja dalam tempoh 7 hari akan dibatalkan dan tindakan tatatertib akan diambil terhadap Kontraktor mengikut syarat-syarat pendaftaran.

b) Jika Kontraktor tidak menyiapkan kerja dalam masa yang ditetapkan, tindakan secara pembayaran gantirugi dan penggantungan lesen dan pendaftaran atau apa-apa cara lain yang difikirkan patut oleh Pegawai Penguasa JPS Negeri Selangor atau wakilnya.

3.
Semua komponen/instrumen/alat yang dibekalkan dan digunakan hendaklah yang baru dan belum dipakai dan mempunyai mutu yang terbaik dan diperolehi dari dalam negara/luar negara (software, firmware dan hardware hendaklah digunapakai seperti sistem sediada di JPS Negeri Selangor dan seperti tertera pada borang sebutharga) serta mendapat kelulusan Pegawai Penguasa JPS Negeri Selangor atau wakilnya. Pegawai tersebut juga mempunyai kuasa untuk meminta contoh-contoh untuk diperiksa sebelum komponen/instrumen/alat tersebut dibekalkan atau digunakan. Semua komponen/instrumen/alat yang dibekalkan hendaklah mempunyai cetakan (stamping) “HAK MILIK KERAJAAN NEGERI SELANGOR” berdakwat kekal.
4.
Hanya pekerja-pekerja yang mahir dalam bidang masing-masing sahaja yang patut digunakan. Kontraktor dan pekerja-pekerjanya hendaklah menjalankan kerja dengan baik dan cermat. Sebarang kerosakan oleh sebab kecuaian pihak Kontraktor atau pekerjanya hendaklah dibaiki atau diganti atas perbelanjaan Kontraktor sendiri.

5. Apabila siap, segala sampah sarap serpihan dan lebihan hendaklah dibersihkan dan dibuang ke tempat yang dibenarkan oleh Pihak Berkuasa Tempatan (PBT).
6. Kontraktor adalah dikehendaki mengambil insuran bagi pekerja (Workmen’s Compensation) atau mencarumkan dengan SOCSO bagi semua pekerjanya.
7.
Komponen/instrumen/alat sedia ada yang diganti/ditukar hendaklah dipulangkan semula ke JPS Negeri Selangor.

8.
Sebarang pertanyaan hendaklah dikemukakan ke Bahagian Pengurusan Banjir dan Reka Bentuk, JPS Negeri Selangor.

1

