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JABATAN PENGAIRAN DAN SALIRAN DAERAH KLANG

TAWARAN SEBUTHARGA JPS/N/KLG/P13/48/2026(SH)






          Sebutharga di keluarkan oleh :







          Ir. Gs. Mohamad Hafiz bin Hassan






          Jurutera Daerah,



 



          Jabatan Pengairan & Saliran Daerah Klang.

TAWARAN : KERJA-KERJA MEMBINA KUARTERS PINTU AIR JALAN PAPAN SERTA KERJA-KERJA BERKAITAN, DAERAH KLANG, SELANGOR DARUL EHSAN
Tawaran ditutup pada 15 JULAI 2026 sebelum 12.00 tengah hari di Jabatan Pengairan dan Saliran Daerah Klang.
	BIL
	PERKARA
	UNIT
	KUANTITI
	KADAR
(RM) 
	JUMLAH
(RM)

	1
	Menyediakan Insuran kerja termasuk Workmen Compensation dan Contractor All Risks bagi kerosakan harta kerajaan, harta benda awam dan perlindungan pekerja (PERKESO) sebelum kerja-kerja dimulakan. 
	Pukal
	 
	 
	

	2
	Mengadakan kos pengangkutan dan penyediaan jentera dan loji semasa dan selepas siap kerja (Mobilisation and Demobilisation)

	Pukal
	 
	 
	

	3
	Menyediakan jentera, peralatan dan tenaga buruh bagi kerja-kerja membersih dan meratakan tapak kuarters pintu air jalan papan serta kerja-kerja berkaitan

	Pukal
	 
	 
	

	4
	Kerja-kerja mengangkut keluar sisa pembersihan tapak kuarters keluar dari tapak ke tempat pembuangan pemborong sendiri serta kerja-kerja berkaitan mengikut arahan Pegawai Penguasa atau wakilnya.

	Pukal
	 
	 
	

	5
	Preparation of documetation and submition of utilities compliance with the legal and apply for all necessary part, licence, etc. including TNB, Air Selangor, IWK, etc..
	Pukal
	 
	 
	

	6
	Establishment of temporary bench marks by qualified and approved Licensed Surveyour including initial, during and final survey for preparation of existing ground profile; as-built plans and any other additional survey; including the use of survey instrumention where for measuring the quantities of any works works executed as approved by the S.O
	Pukal
	 
	 
	

	7
	Survey and setting out by licened surveyor
	Pukal
	 
	 
	

	8
	Membekal, merata dan memadat tanah merah jenis laterite di tapak termasuk kerja memadat menggunakan Vibrating Roller seberat 8 tan sebanyak 3 kali laluan serta kerja-kerja berkaitan. 
	M³
	200
	
	

	 
	Jumlah dibawa ke m/s sebelah
	


KADAR


JUMLAH

	(RM)

	 
	Jumlah dibawa dari m/s sebelah
	

	9
	Kerja-kerja membina kuarters baru Pintu Jalan Papan mengikut No Plan : JPS/N/KLG/P13/48/2026(SH)/MS1 sehingga MS10
	 
	 
	 
	 

	 
	PILING AND EQUIPMENT
	 
	 
	 
	 

	10
	Provision of all necessary piling plant and equipment, transportation to the Site, handling, assembling, and removal off the Site after completion of operation.

	SUM

	 
	 
	

	11
	Moving and handling of all piling plant and equipment within the Site and from location to location as often as sumis, and whenever necessary for the execution of the whole piling operation.

	SUM

	 
	 
	

	 
	REINFORCED CONCRETE PILES
	 
	 
	 
	 

	 
	Note to Tenderers :
The measurement of piling shall be in accordance with the following :
i)The piles shall be 175mm x 175mm precast
reinforced concrete piles; Grade 40 or as specified in the drawings and specification.
ii)Supply of initial and extension pile are billed
separately in linear meter.
iii)Prices for piles shall include for casting them either on or of site and all necessary formwork including forming necessary recess etc. reinforcement, lifting tongles, pile shoes or extension base plate andextension cap plates all as described.
iv)Prices for handling, transporting, pitching and driving of piles shall be deemed to include the provision of all necessary piling equipment and other plant on site and dismantling and removing the same on completion of the piling work.
v)Prices for testing of piles shall be deemed to include the provision of all pile testing equipment on site and dismantling and removing the same on completion of the piling work.
	 
	 
	 
	 

	 
	vi)The pay length for the driving of each pile shall be the actual penetration of the pile into the ground.                                                                                           vii)The Contractor shall take note that not withstanding to term of Conditions of Contract, the quantities of piling works in this bill are 'PROVISIONAL' and subject to re-measurement.

	 
	 
	 
	 

	 
	Jumlah dibawa ke m/s sebelah
	


KADAR


JUMLAH

	(RM)

	 
	Jumlah dibawa dari m/s sebelah
	 

	12
	200mm x 200mm concrete G40 square precast reinforced concrete piles

	 
	 
	 
	 

	13
	Supply initial piles with mild steel pointed shoes of 6m length.
i) Quarters
	Nr

	31

	
	

	14
	Supply extension piles of 6m length
i) Quarters
	Nr

	62

	
	

	15
	Depth driven single or cluster; hydraulic hammerincluding handle, transport and pitch.
i) Quarters
	M

	558

	
	

	16
	Jointing with 10mm fillet weld all around connecting edges of joint plates including covering weld with cold bitumen.
	Nr

	62

	
	

	 
	i) Quarters
	 
	 
	
	

	17
	Cut-off 200mm x 200mm piles. The rate shall be include preparing of pile head.
	Nr

	31

	
	

	 
	i) Quarters
	 
	 
	
	

	 
	PILE TESTS
	 
	 
	
	

	18
	PDA test on 175mm x 175mm precast reinforced concrete square pile.
	Nr

	2

	
	

	 
	
	 
	 
	
	

	 
	BUILDING WORKS
	 
	 
	 
	 

	 
	(refer Dwg No. )
	 
	 
	 
	 

	 
	EXCAVATION
	 
	 
	 
	 

	 
	Cut and Dispose
	 
	 
	 
	 

	19
	Excavation in earth material general surface commencing from original ground level to platform level to disposal site approved by the S.O.
	M3

	109

	
	

	 
	
	 
	 
	
	

	 
	IN SITU CONCRETE DESIGN MIX
	 
	 
	
	

	 
	Grade: C15 Concrete
	 
	 
	
	

	20
	Blinding mass concrete, 50mm thick under pilecaps, ground beams, ground slabs and the likes.
	M2

	188

	
	

	 
	Grade: C30 Concrete
	 
	 
	
	

	21
	Reinforced concrete to pile cap, ground beam, ground slabs, columns, roof beams and the likes.
	M3

	52

	
	

	 
	FORMWORK
	 
	 
	
	

	 
	Sides and Soffits
	 
	 
	
	

	22
	F1: rough finish to pile cap, stump, beams, slab, columns and the likes.
	M2

	321

	
	

	 
	
	 
	 
	 
	 

	 
	
	
	
	
	 
	 
	 
	 

	 
	Jumlah dibawa ke m/s sebelah
	


KADAR


JUMLAH

	(RM)

	 
	Jumlah dibawa dari m/s sebelah
	 

	 
	REINFORCEMENT
	 
	 
	 
	 

	 
	
	
	
	
	 
	 
	 
	 

	 
	Mild Steel Bars & High Tensile Bars
	 
	 
	 
	 

	23
	Nominal diameter: 10mm high tensile bars.
	kg
	1031
	
	

	24
	Nominal diameter: 12mm high tensile bars.
	kg
	1618
	
	

	25
	Nominal diameter: 16mm high tensile bars.
	kg
	353
	
	

	26
	High tensile steel fabric –  mesh A252 (A8),
	M2
	295
	
	

	 
	4.15kg/m2 (measure nett - no allowance made for lap).

	 
	 
	
	

	 
	BRICKWORK
	 
	 
	
	

	 
	Vertical Straight Walls
	 
	 
	
	

	27
	110mm thick common claybrickwork laid on cement and sand mortar (1:3) mortar with an approved plasticiser as described including layer of exmet at every fourth courses as described.


	M2

	171

	
	

	 
	ROOFING WORK
	 
	 
	
	

	 
	Roof Structure
	 
	 
	
	

	 
	Metal of stated roofing system and components to be designed by the contractor.
	 
	 
	
	

	 
	
	 
	 
	
	

	28
	Design, supply and install light weight trusses including all related truss member such as top chord, bottom chord, purlin, web etc and fixing into position and manufactor's instruction, material and design warranty and to Engineer's and S.O's approval. The design must done with Professional Engineer endorsement, who is to approve and sign all the drawing, design calculation, and submission to S.O (measure flat on plan).

	M2

	130

	
	

	 
	Roof Covering
	 
	 
	 
	 

	29
	Interlocking concrete roofing tiles as per specification laid to 30 degree to the horizontal to Engineer's drawing.

	M2

	130

	
	

	 
	Rate to include 25mm PU foam, ridge, hid, valley, flashing, end caps and other accessary as per S.O's satisfaction (measure flat on plan).

	 
	 
	
	

	 
	
	 
	 
	
	

	
	Jumlah dibawa ke m/s sebelah

	


KADAR


JUMLAH

	(RM)


	 
	Jumlah dibawa dari m/s sebelah

	

	 
	WINDOWS AND DOORS
	 
	 
	
	

	 
	Doors
	
	
	 
	 
	
	

	30
	750mm x 2100mm single leaf hardwood

laminated flush door panel with aluminium frames and approved ironmongery, jointing materials and other accessories and including approved timber and metal paint finish to all exposed surfaces.

	Nr
	2
	
	

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	31
	900mm x 2100mm single leaf hardwood

laminated flush door panel with aluminium frames and approved ironmongery, jointing materials and other accessories and including approved timber and metal paint finish to all exposed surfaces.
	Nr
	5
	
	

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	Windows
	 
	 
	 
	 

	32
	1200 mm x 1200 mm natural anodised aluminium side hung casement window complete with 6 mm thick clear float glass as per drawing.
	Nr
	2
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	33
	1800 mm x 1200 mm natural anodised aluminium side hung casement window complete with 6 mm thick clear float glass as per drawing.
	Nr
	5
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	34
	600 mm x 1200 mm natural anodised aluminium top hung casement window complete with 6 mm thick clear float glass as per drawing.
	Nr
	2
	
	

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	FINISHES
	 
	 
	 
	 

	 
	Floor Finishes
	 
	 
	 
	 

	 
	Rate for floor finishes to include fixing, supply of fixing components, drilling or cutting of associated work, preparing surfaces, forming joints, mitres, angles, fillets, built-up edges, and laying to chambers or falls.
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	35
	Homogeneous tiles; 300 x 300 x 7.6 mm thick. Rate to include cement mortar screed.


	M2
	98
	
	

	 
	
	 
	 
	
	

	36
	Non-slip ceramic tiles; 200mm x 200mm x 7 mm thick. Rate to include cement mortar screed.
	M2
	10
	
	

	 
	
	 
	 
	 
	 

	 
	Wall Finishes
	 
	 
	 
	 

	37
	19mm thick cement and sand (1:6) mixed with and approved plasticiser with wooden float at plainface walls,beams, columns and the likes.


	M2

	393

	
	

	
	Jumlah dibawa ke m/s sebelah

	


KADAR


JUMLAH

	(RM)


	 
	Jumlah dibawa dari m/s sebelah

	

	
	Ceiling Finishes

Concealed ceiling of approved texture and cut to size as specified including light through, at necessary joints anti up lift insert rod on timber frame fixed in accordance to manufacturer's instructions all as per S.O's satisfaction.

	
	
	
	

	38
	600mm x 1200mm x 3.2mm Thick 'UAC' superflex or other equal and approved suspended non asbestos sheet not exceeding 3.50m.

	M2
	130
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	 
	EMULSION PAINT OR ACRYLIC PAINT
	 
	 
	
	

	 
	Prepare and apply one coat of sealer and two coats of approved emulsion paint to:
	 
	 
	
	

	 
	
	 
	 
	
	

	39
	Smooth plastered surfaces of internal walls, beams, columns and the likes.
	M2
	267
	
	

	 
	
	 
	 
	
	

	 
	Prepare and apply one coat of sealer and two coats of approved acrylic weather shield paint to:
	 
	 
	
	

	 
	
	 
	 
	
	

	40
	Smooth plastered surfaces of external walls, beams, columns and the likes.
	M2
	126
	
	

	 
	
	 
	 
	
	

	 
	
	
	
	
	 
	 
	
	

	 
	PLUMBING WORK
	 
	 
	
	

	 
	Sanitary Appliances and Fittings
	 
	 
	
	

	41
	Water closets; Claytan 404 or approved equivalent 6-litre single flush side lever, bottom inlet overflow cistern with flapper valve internal fittings including medium duty plastic seat and cover.

	Nr
	2
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	Septic Tanks
	 
	 
	 
	 

	 
	Rate for septic tanks shall be deemed to include foundation, excavation, upholding sides of excavation, bedding, installation, backfilling, and all other related works where expressly required.

	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	42
	Septic tank for five population equivalent (5 PE) with a minimum of 24 hours of hydraulic retention time and a dual size aggregate down flow filter media.

	Nr
	1
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	 
	SUMP/ INSPECTION CHAMBER
	 
	 
	
	

	43
	Precast concrete; 750 mm x 750 mm x 750 mm deep including all assocceries to complete the work.

	Nr
	1
	
	

	 
	
	 
	 
	 
	 

	
	Jumlah dibawa ke m/s sebelah

	


KADAR


JUMLAH

	(RM)


	 
	Jumlah dibawa dari m/s sebelah

	

	 
	DRAINAGE
	 
	 
	 
	 

	 
	Item for drainage shall deemed to include excavation,cement jointing, sand, formworks, reinforcement works and concrete beddings, crusher run, concrete base, BRC, shuttering, struts, weepholes, allow for connection and all accessory and associated works to complete the works.
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	44
	Excavation in earth for 225mm precast HRGW, depth not exceeding 300mm.


	M
	51
	
	

	 
	
	 
	 
	
	

	45
	Supply and complete 450mm x 450mm brick sump with plaster and cover.


	Nr
	1
	
	

	 
	
	 
	 
	
	

	46
	Supply and install 225mm precast HRGW drain.


	M

	47

	
	

	47
	Supply and install 250mm diameter concrete culvert type Class 'Z'.


	M
	4
	
	

	 
	
	 
	 
	
	

	48
	Excavation in earth for precast U-drain, depth not exceeding 1000mm.
	M
	5
	
	

	 
	
	 
	 
	
	

	49
	Supply and conplete 450mm x 450mm precast U-drain.


	M

	5

	
	

	 
	ROADS AND PAVING
	 
	 
	
	

	 
	Sub-Grade Preparation
	 
	 
	
	

	50
	Preparation of formation as specified and as directed by the S.O for receiving road pavement as per ATJ 5/85, revision 2013, minimum CBR 12.1%.


	M2
	100
	
	

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	Roadbase
	 
	 
	 
	 

	 
	Roadbase shall be deemed to include chamfer.

	 
	 
	 
	 

	51
	Supply, deliver, spread, grade and compact 300mm thick road base material with complying maximum 10% fines as per standard specification.

	M
	100
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	 
	Dense Bituminuous Macadam
	 
	 
	
	

	52
	Regulating bituminous macadam binder course BMB 20 to the required formation level.

	M
	100
	
	

	 
	
	 
	 
	 
	 

	 
	Jumlah dibawa ke m/s sebelah

	


KADAR


JUMLAH

	(RM)

	 
	Jumlah dibawa dari m/s sebelah
	

	 
	MECHANICAL AND ELECTRICAL WORKS
	 
	 
	 
	 

	 
	(refer Dwg No. )
	 
	 
	 
	 

	 
	
	
	
	
	 
	 
	 
	 

	 
	ELECTRICAL SYSTEM
	 
	 
	 
	 

	 
	To supply, install, testing and commissioning to use the following as per drawing and specifications. All quantities given are PROVISIONAL. The actual quantities installed 

shall be measured on site after completion and prices adjusted accordingly.
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	Wiring
	
	 
	 
	 
	 

	 
	All wiring shall be in uPVC heavy duty consuit (BS EN 50086-2-1: 1996 4421) / G.I. conduit at top level / hot dipped galvanised trunking.
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	Concealed Wiring Works
	 
	 
	 
	 

	53
	Lighting point using 2 x 1.5 mm sq PVC & protective conductor c/w 10A 1 way SP flush switch.
	Nr
	14
	
	

	 
	
	 
	 
	
	

	54
	Ceiling fan point using 2 x 1.5 mm sq PVC & protective conductor 10A SP flush switch and hook.
	Nr
	5
	
	

	 
	
	 
	 
	
	

	55
	13A socket outlet point using 2 x 2.5 mm sq PVC cable & protective conductor c/w 13A 1 gang 3 pin flush switched socket.
	Nr
	10
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	56
	Air cond point using 2 x 4 mm sq PVC cable & protective conductor c/w 15A switch with neon indicator light and 15A round 3 pin socket outlet.
	Nr
	2
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	 
	Luminaires and Equipment
	 
	 
	
	

	 
	Surface Luminaire
	 
	 
	
	

	57
	1 x 36W LED Bare Channel Fitting (T8) c/w switches and all accessories at ceiling.
	Nr
	10
	
	

	 
	
	 
	 
	
	

	58
	1 x 36W LED Bare Channel Fitting (T8) c/w switches and all accessories at wall.
	Nr
	4
	
	

	 
	
	 
	 
	
	

	59
	Ceiling fan with 1500 diameter c/w switches, fittings and all accessories.
	Nr
	5
	
	

	 
	
	 
	 
	
	

	 
	Distribution Board
	 
	 
	
	

	60
	To supply and install the 63A SPN c/w MCBs, MCCB and RCCBs etc. as per drawing.

	Nr
	1
	
	

	 
	
	 
	 
	
	

	61
	To supply and install TNB meter panel c/w connection cable as per drawing.

	Nr
	1
	
	

	 
	
	 
	 
	 
	 

	
	Jumlah dibawa dari m/s sebelah

	


KADAR


JUMLAH

	(RM)

	 
	Jumlah dibawa dari m/s sebelah

	

	
	Earthing System
	
	
	
	

	62
	Supply, install, testing and commissioning solid earthing system using 25mm x 3mm copper tape, earthing terminal, copper jacketed steel core rod with 16mm diameter x 2 nos. 1500mm length, precast heavy duty

inspection chamber and related accessories until meet the reading less than 3 ohms as per drawing and specification.

(Connection of the earthing conductors to the earth electrodes shall be by Exothermic Welding Connections)

	Sum
	 
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	 
	Telephone System
	 
	 
	
	

	63
	1-way of 100mm dia. uPVC duct Class D c/w draw wire from telephone pit to external.

	Sum
	 
	
	

	 
	
	 
	 
	
	

	64
	Fibre termination box c/w surge arrestor including earthing.

	Nr
	1
	
	

	 
	
	 
	 
	
	

	65
	Telephone point inclusive of wall socket (RJ11) c/w wiring using 2 pairs 0.63mm tel. in uPVC heavy duty conduit including testing.

	Sum
	 
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	66
	Wiring using CAT6 cable for RJ45 socket at living room in consealed conduit c/w RJ45 faceplate and testing.
	Sum
	 
	
	

	 
	
	 
	 
	
	

	 
	MATV System
	 
	 
	
	

	67
	Wiring using RG11 coaxial cable in uPVC heavy duty c/w TV/FM socket point (flush type) including connector and other accessories.
	Sum
	 
	
	

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	Others Work
	 
	 
	 
	 

	68
	Any other items, works or costs not specified above but is shown in the drawing or included in the scope of works and/or specification, or deemed necessary for the full and proper execution and completion of this element

(please specify):-
	Sum
	 
	 
	

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	i)
	
	
	
	 
	 
	 
	 

	 
	ii)
	
	
	
	 
	 
	 
	 

	 
	iii)
	
	
	
	 
	 
	 
	 

	 
	COLD WATER AND SANITARY PLUMBING SYSTEM
	 
	 
	 
	 

	 
	The scope of works shall include call for testings, supply supply, installation and commissioning of the complete Cold Water and Sanitary Plumbing installation as per

drawing and this bill of quantities comprising of but not necessary limited to the following.

	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	
	Jumlah dibawa dari m/s sebelah

	


KADAR


JUMLAH

	(RM)

	 
	Jumlah dibawa dari m/s sebelah

	

	 
	Cold Water Services (Rumah Sesebuah 1 Tingkat)
	 
	 
	 
	 

	 
	Supply and install all material for a complete

mechanical system as per specification and drawings.
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	Bath 1 and Bath 2
	 
	 
	 
	 

	69
	To supply and install incoming 100mm diameter underground MSCL pipe from external water reticulation,1 no. of water meter c/w stainless steel, stand up pipe, hot tapping from Air Selangor main pipe and other

accessories required by Local Authorities.

	Nr
	1
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	70
	Incoming 25mm diameter underground HDPE pipe from water meter to poly tank and kitchen.
	Nr
	1
	
	

	 
	
	 
	 
	
	

	71
	To supply and install poly storage tank c/w tank support, valves, copper ball float, overflow and scour pipe and necessary accessories required by Local Authories.

Roof tank - capacity : 220 gallons
	Nr
	2
	
	

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	72
 
	To supply and install the distribution pipes from water tank to fittings as per drawings.

i) 20mm diameter PPR pipe.

ii) 25mm diameter PPR pipe.
	 
	 
	 
	 

	
	
	 
	 
	 
	 

	 
	
	Lot
	1
	
	

	 
	
	Lot
	1
	
	

	73
	All valves and fittings such as tees, bends, stop cocks, strainers and all accessories to complete the work.
	Lot
	1
	
	

	 
	
	 
	 
	
	

	74
	Connection of supply pipe to fittings such as taps, WC sink, basin, shower and other related fittings to complete the work. 

	Lot
	1
	
	

	 
	
	 
	 
	 
	

	 
	
	 
	 
	 
	

	75
	Flushing of cold water systems of debris, dirts and other chemical and foreign material to ensure proper water as per standard and specification.
	Sum
	 
	 
	

	 
	
	 
	 
	 
	

	 
	
	 
	 
	 
	

	 
	
	
	
	
	 
	 
	 
	

	 
	Other Items 
	 
	 
	 
	

	76
	To arrange for inspection until up to Consultant and S.O's satisfaction.

	Sum
	 
	 
	

	 
	
	 
	 
	 
	

	77
	To arrange and liase with relevant authorities and JBA inspection for the whole installation until final clearance is obtained.

	Sum
	 
	 
	

	 
	
	 
	 
	 
	

	 
	
	 
	 
	 
	

	78
	Testing and commisioning.

	Sum

	 
	 
	

	79
	Monthly comprehensive maintenance during defects liability period (DLP).

	Sum
	 
	 
	

	 
	
	 
	 
	 
	 

	
	Jumlah dibawa dari m/s sebelah

	


KADAR


JUMLAH

	(RM)

	 
	Jumlah dibawa dari m/s sebelah

	

	80
	Any other items, works or costs not specified above but is shown in the drawing or included in the scope of works and/or specification, or deemed necessary for the full and proper execution and completion of this element
	Sum
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	(please specify):-
	 
	 
	 
	 

	 
	i)
	
	
	
	 
	 
	 
	 

	 
	ii)
	
	
	
	 
	 
	 
	 

	 
	iii)
	
	
	
	 
	 
	 
	 

	 
	DOMESTIC SANITARY PLUMBING SERVICES
	 
	 
	 
	 

	 
	The scope of works shall include call for testings, supply, installation and commissioning of the complete Domestic Sanitary Plumbing installation as per drawing and this bill of quantities comprising of but not necessary limited to the following.
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	81
	32mm diameter uPVC brown pipe c/w 75mm water seal depth, from basin to floor trap c/w bottle trap, fitting, bedding, backfilling and all accessories to complete the work.
	Lot
	1
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	82
	75mm diameter uPVC brown pipe from floor trap to gully trap c/w stainless steel grating, 50 mm water seal depth, fitting, bedding, backfilling and all accessories to complete the work (gradient 1 : 300).
	Lot
	1
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	83
	100mm diameter uPVC brown pipe from gully trap to manhole c/w fitting, bedding, backfilling and all accessories to complete the work (gradien 1 : 300).
	Lot
	1
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	84
	100mm diameter uPVC brown pipe from water closet to manhole c/w 50mm water seal depth, fitting, bedding, backfilling and all accessories to complete the work.
	Lot
	1
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	 
	 

	85
	100mm diameter uPVC brown pipe from dropper to manhole c/w 135º radius bend fitting, bedding, backfilling and all accessories to complete the work.
	Lot
	1
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	86
	Dropper pipe consist of 100mm diameter uPVC soil and waste pipe, 100mm diameter uPVC vent pipe, termination of 100mm diameter UPVC vent pipe to main 100mm diameter UPVC soil and waste pipe at roof, vent cowl at 450mm above roof, necessary fitting and all accessories to complete the work.
	Lot
	1
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	87
	Installation of gully trap c/w cover to suit floor tile and other accessories to complete the work.
	Nr
	3
	
	

	 
	
	 
	 
	
	

	88
	Connections of fitting to waste pipe such as sink, basin,WC and other related fitting c/w necessary connections and all accessories to complete the work.
	Lot
	1
	
	

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	Jumlah dibawa ke m/s sebelah
	 


KADAR


JUMLAH

	(RM)

	 
	Jumlah dibawa dari m/s sebelah
	 

	89
	Installation of floor traps c/w stainless steel grating /fitting and all accessories to complete the work.
	Nr
	3
	
	

	 
	
	 
	 
	
	

	 
	
	
	
	
	 
	 
	
	

	90
	Installation of vent cowls at roof top c/w necessary fitting and all accessories to complete the work.
	Nr
	2
	
	

	 
	
	 
	 
	
	

	 
	
	
	
	
	 
	 
	
	

	 
	EXTERNAL SANITARY PLUMBING WORKS
	 
	 
	
	

	 
	
	
	
	
	 
	 
	
	

	91
	Excavation, supply and lay sewerage 150mm Upvc brown pipe, c/w fitting, bedding, backfilling and all accessories to complete the work.
	Lot
	1
	
	

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	
	
	
	 
	 
	 
	 

	92
	Depth 900mm to 1500mm, 600mm x 600mm

underground inspection chamber c/w heavy duty manhole cover (written 'IWK Emboss').

	Lot
	3
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	 
	
	
	
	
	 
	 
	
	

	93
	Cleaning of sanitary system of debris, dirt, sand and other chemical and foreign material to ensure proper sewerage and sanitary as per standard and specification.
	Sum
	 
	
	

	 
	
	 
	 
	
	

	 
	
	 
	 
	
	

	 
	
	
	
	
	 
	 
	
	

	94
	To arrange for inspection until up to Consultant and S.O's satisfaction.

	Sum
	 
	
	

	 
	
	 
	 
	
	

	 
	
	
	
	
	 
	 
	
	

	95
	Testing and commisioning.
	Sum
	 
	
	

	 
	
	
	
	
	 
	 
	 
	 

	 
	OTHER WORK
	 
	 
	 
	 

	96
	Any other items, works or costs not specified above but is shown in the drawing or included in the scope of works and/or specification, or deemed necessary for the full and proper execution and completion of this element
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	
	 
	 
	 
	 

	 
	(please specify):-
	 
	 
	 
	 

	 
	i)
	
	
	
	 
	 
	 
	 

	 
	ii)
	
	
	
	 
	 
	 
	 

	 
	iii)
	
	
	
	 
	 
	 
	 

	 97
	Membekal dan memasang Pintu Pagar utama jenis dua daun  bersaiz 2.1m tinggi 2.4m lebar pintu (Hot Dipped Galvanised BD 729) dengan ibu dan anak kunci serta kerja-kerja berkaitan.

	nos
	1
	 
	 

	98
	Membekal dan memasang Pintu Pagar utama jenis dua daun  bersaiz 2.1m tinggi 1m lebar pintu (Hot Dipped Galvanised BD 729) dengan ibu dan anak kunci serta kerja-kerja berkaitan.

	nos
	1
	
	

	
	Jumlah dibawa ke m/s sebelah

	


KADAR


JUMLAH

	(RM)

	
	Jumlah dibawa dari m/s sebelah
	

	99
	Menyediakan 2 salinan laporan bergambar (berwarna dan bertarikh) yang menunjukkan kemajuan kerja-kerja sebelum, semasa dan selepas siap kerja dalam bentuk hardcopy dan  soft copy  (pendrive).

Nota: Kontraktor bertanggungjawab terhadap sebarang kerosakan kemudahan awam atas sifat kelalaian dan perlu diperbaiki segera. Pemotongan bayaran akhir akan dilakukan sekiranya kerosakan tersebut tidak dibaiki.
	Pukal
	 
	 
	

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 Jumlah Keseluruhan
	 


Tempoh siap kerja :  Tiga (3) bulan
Syarat-Syarat : -
A) Pemborong perlu memahami dengan teliti dan melaksanakan segala syarat syarat yang dilampirkan.

B) Pemborong perlu meyediakan laporan bergambar sebelum dan selepas kerja-kerja pembinaan.

C) Segala harga yang dinyatakan hendaklah merangkumi tempoh yang ditetapkan.

Ringgit Malaysia

………………………………………………………………………………………………
………………………………………………………………………………………………
Tandatangan Pemborong………………...... Tandatangan Saksi     : ………….............
    Nama Penuh Pemborong …………………  Nama Saksi                 : ………………….
    No Kad.Pengenalan      : ………….......       No. Kad Pengenalan   : ……………….....
 No. Tel                  : …………………             No. Tel                        : ………………….                                                                          
Cop Syarikat
------------------------------
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